**Connecting B228 to Bosch 4000**

When connecting the **B228** expander to a Bosch 4000, there are module addresses to consider. If using addresses **2** and **3** for zones **17 – 24** and zones **25 – 32** the zones are automatically assigned to the **B228** expanders.

If B228 expander is adressed 1 for zones 9 – 16 you must reassign the zones form the panel to use the expander zones. This can only be done withy A-Link Plus software v 1.21.

Control panel configuration - Zone Config – Zone Source

A white screen with black lines

AI-generated content may be incorrect.

By default, zones 9 – 16 are assigned to the panel in zone doubling configuration. If using the B228 expanders zone doubling is no longer available.